{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["調査結果"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"調査結果","index":0,"n_rows":48,"n_cols":24,"rows_kept":48,"cut":false,"hidden":false,"merged":[[1,19,1,20],[0,16,2,16],[0,17,2,17],[0,18,0,23],[0,0,2,0],[0,1,0,15],[1,1,2,1],[1,2,1,4],[1,5,1,7],[1,8,2,8],[1,9,2,9],[1,13,2,13],[1,14,2,14],[1,15,2,15]],"flags":["formulas_cached_only"]}
["地点番号","現地調査",{"$nulls":14},"調査グループ","備考","潮位補正"]
[null,"地名","北緯",null,null,"東経",null,null,"年/月/日","時刻","測定高*3","津波高","汀線からの","測定対象","根拠","信頼度*2",null,null,"測定時の","最大波発生日時（予想）",null,"最大波発生時（予想）","潮位補正の","潮位補正後の高さ"]
[null,null,"度","分","秒","度","分","秒",null,null," a (m)","の種類*1","測定距離 (m)",{"$nulls":5},"潮位 b (m)","年/月/日","時刻","の潮位 c (m)","参照地点","a+b-c (m)"]
[1,"宮城県亘理町荒浜地区",38,2,32.82,140,55,10.02,"2011-04-06","11:00:00",7.66,"I",185.09,"荒浜雨水ポンプ場","浸水痕","A","農工研","デジタルレベル測量",0.03,"2011-03-11","15:30:00",0.43,"仙台塩釜港",7.260000000000001]
[2,"宮城県亘理町牛橋排水機場",37,59,17.304,140,54,23.112,"2011-04-06","14:20:00",5.45,"I","20.87（海と通じていると思われる水面からの距離）","牛橋排水機場","浸水痕","A","農工研","デジタルレベル測量",0.57,"2011-03-11","15:30:00",0.43,"仙台塩釜港",5.590000000000001]
[3,"宮城県南三陸町波伝谷海岸",38,38,36.24,141,28,51.78,"2011-04-07","13:30:00",13.02,"I",43.76,"波伝谷海岸堤防の直背後","漂着物","A","農工研","デジタルレベル測量",0.28,"2011-03-11","15:30:00",0.43,"大船渡",12.87]
[4,"宮城県南三陸町波伝谷海岸",38,38,34.8,141,28,49.548,"2011-04-07","13:50:00",12.97,"R",139.64,"波伝谷海岸背後の道路","漂着物","A","農工研","デジタルレベル測量",0.34,"2011-03-11","15:30:00",0.43,"大船渡",12.88]
[5,"岩手県陸前高田市小友農地海岸",38,59,36.6,141,40,43.104,"2011-04-08","11:35:00",13.79,"I",null,"海岸堤防脇の海岸線に面した斜面","漂着物","A","農工研","レーザー距離計による計測",0.09,"2011-03-11","15:30:00",0.43,"大船渡",13.45]
[6,"岩手県釜石市本郷農地海岸",39,12,34.236,141,53,16.98,"2011-04-08","15:44:00",13.08,"I",null,"海岸堤防脇の海岸線に面した斜面","漂着物","A","農工研","レーザー距離計による計測（浸水深）"]
[7,"岩手県山田町小谷鳥農地海岸",39,25,39.72,142,0,48.312,"2011-04-09","14:40:00",12.7,"I",null,"海岸堤防脇の海岸線に面した斜面","漂着物","A","農工研","レーザー距離計による計測（浸水深）"]
[8,"宮城県松島町宮戸島",38,21,12.672,141,9,25.56,"2011-04-05","18:02:00",5.96,"I",190,"松ヶ島橋脇の高床式倉庫","漂着物＋浸水痕","A","農工研","レーザー距離計による計測",1.16,"2011-03-11","15:30:00",0.43,"仙台塩釜港",6.69]
{"$rows_empty":13}
["*1 津波高の種類",{"$nulls":15},"氏　名","所　属"]
["　　R: 遡上高",{"$nulls":14},"○","丹治　肇","農業・食品産業技術総合研究機構農村工学研究所"]
["　　I: 浸水高（浸水深を測定した場合は備考欄に入力してください．）",{"$nulls":15},"中矢哲郎","農業・食品産業技術総合研究機構農村工学研究所"]
["　　P: 港内津波高（港湾において，岸壁は越えてはいないが明確に高さが分かる津波）",{"$nulls":15},"松島健一","農業・食品産業技術総合研究機構農村工学研究所"]
["　　W: 微弱な津波（常時波浪との判別が不可能な微弱な津波）",{"$nulls":15},"桐　博英","農業・食品産業技術総合研究機構農村工学研究所"]
["*2 信頼度の判断基準"]
["　　A: 信頼度大なるもの。痕跡明瞭にして，測量誤差最も小なるもの。"]
["　　B: 信頼度中なるもの。痕跡不明につき，聞き込みにより，周囲の状況から信頼ある水位を知るもの。測量誤差小。"]
["　　C: 信頼度小なるもの。その他砂浜などで異常に波がはい上がったと思われるもの，あるいは測点が海辺より離れ測量誤差が大なるもの。"]
["　　D: 信頼度極小なるもの。高潮，台風などの影響で痕跡が重複し，不明瞭なもの，等。"]
["*3 GPS測量の場合は標高値を入力する．その際，備考欄に測定機器（例えば，Garmin, VRS-GPS, ProMark3など）および可能であれば測位精度等の補足情報を入力する．"]
["　測定点の写真（できればGPSカメラで）を撮影しておくこと．"]
{"$rows_empty":11}
[{"$nulls":16},"※代表者の氏名に◯を付ける．"]