{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["調査結果"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"調査結果","index":0,"n_rows":101,"n_cols":24,"rows_kept":101,"cut":false,"hidden":false,"merged":[[0,0,2,0],[0,1,0,15],[1,1,2,1],[1,2,1,4],[1,5,1,7],[1,8,2,8],[1,9,2,9],[1,13,2,13],[1,14,2,14],[1,15,2,15],[1,19,1,20],[0,16,2,16],[0,17,2,17],[0,18,0,23]],"flags":["formulas_cached_only"]}
["地点番号","現地調査",{"$nulls":14},"調査グループ","備考","潮位補正"]
[null,"地名","北緯",null,null,"東経",null,null,"年/月/日","時刻","測定高","津波高","汀線からの","測定対象","根拠","信頼度*2",null,null,"測定時の","最大波発生日時（予想）",null,"最大波発生時（予想）","潮位補正の","潮位補正後の高さ"]
[null,null,"度","分","秒","度","分","秒",null,null," a (m)","の種類*1","測定距離 (m)",{"$nulls":5},"潮位 b (m)","年/月/日","時刻","の潮位 c (m)","参照地点","a+b-c (m)"]
["MG01-1","仙台港臨港団地①",38,15,47.46,140,59,13.56,"2011-03-19","13:07:00",1.15,"I",2620,"道路南側街灯","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",2.59]
["MG01-2","仙台港臨港団地②",38,15,46.91,140,59,13.09,"2011-03-19","13:08:00",0.95,"I",2620,"スーパーハウス屋さん","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",2.39]
["MG01-3","仙台港臨港団地③",38,15,47.16,140,59,12.18,"2011-03-19","13:10:00",1.4,"I",2640,"スーパーハウス屋さん","草","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",2.84]
["MG01-4","仙台港臨港団地④",38,15,46.02,140,59,17.8,"2011-03-19","13:14:00",1.4,"I",2470,"道路に駐車中の四駆車（車高1.84m）のドアミラー上","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",2.84]
["MG01-5","仙台港臨港団地⑤",38,15,46.34,140,59,18.02,"2011-03-19","13:14:00",0.67,"I",2510,"道路北側（自販機）","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",2.11]
["MG02-1","通行監視カメラ",38,15,2.16,140,59,9.9,"2011-03-19",40621.57237268519,2.6,"R",1910,"道路監視カメラ支柱","草","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",4.04]
["MG02-2","通行監視カメラ",38,15,2.16,140,59,9.9,"2011-03-19",40621.57237268519,1.35,"I",1910,"道路監視カメラ支柱","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",2.79]
["MG03-1","住宅近傍電柱",38,15,3.610799999989922,140,59,9.902400000019043,"2011-03-19",40621.57392361111,1.6,"I",1930,"電柱","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.04]
["MG03-2","住宅",38,15,4.02,140,59,10.26,"2011-03-19",40621.57440972222,2.2,"I",1940,"住宅壁面","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.64]
["MG03-3","セブンイレブン",38,15,4.36,140,59,9.23,"2011-03-19",40621.5750462963,1,"I",1950,"店舗壁面","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",2.44]
["MG04-1","仙台市岡田ポンプ場",38,14,56.690368799988846,140,59,19.680176399967877,"2011-03-19",40621.58090277778,2.6,"I",1630,"南面","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",4.04]
["MG04-2","仙台市岡田ポンプ場",38,14,56.965027199999554,140,59,20.119628399979774,"2011-03-19",40621.58179398148,2.65,"I",1620,"東面中央","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",4.09]
["MG04-3","仙台市岡田ポンプ場",38,14,57.433200000008924,140,59,20.504399999956604,"2011-03-19",40621.582291666666,2.85,"I",1630,"東面北","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",4.29]
["MG04-4","仙台市岡田ポンプ場",38,14,57.541808400004015,140,59,20.339354400036882,"2011-03-19",40621.5831712963,3.4,"I",1630,"北面","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",4.840000000000001]
["MG04-5","仙台市岡田ポンプ場",38,14,57.70660559999271,140,59,19.460450400013087,"2011-03-19",40621.58387731481,1.8,"I",1640,"西面","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.2399999999999998]
["MG04-6","仙台市岡田ポンプ場向かい電柱",38,14,55.8,140,59,20.82,"2011-03-19",40621.58557870371,1.6,"I",1590,"電柱","シミ","B","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.04]
["MG05-1","仙台市南蒲生浄化センター",38,14,59.009999999992715,141,0,9.338399999955982,"2011-03-19",40621.593125,1.3,"I",650,"建屋南壁面","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",3.4,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",5.140000000000001]
["MG05-2","仙台市南蒲生浄化センター",38,15,0.7703999999989719,141,0,9.669600000040646,"2011-03-19",40621.594513888886,1.5,"I",670,"フェンス","草","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",3.2,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",5.140000000000001]
["MG05-3","仙台市南蒲生浄化センター",38,14,58.73639999999284,141,0,10.929600000031314,"2011-03-19",40621.59699074074,3.6,"I",620,"建屋東壁面","傷","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",3.4,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",7.44]
["MG05-4","仙台市南蒲生浄化センター",38,14,58.145999999999844,141,0,15.82199999995737,"2011-03-19",40621.599444444444,3.1,"I",510,"建屋西壁面","草混じり泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",3.6,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",7.140000000000001]
["MG05-5","仙台市南蒲生浄化センター",38,14,57.994799999997895,141,0,19.720800000038707,"2011-03-19",40621.60241898148,3.7,"I",440,"建屋西壁面","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",3.6,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",7.740000000000001]
["MG05-6","仙台市南蒲生浄化センター",38,14,59.60040000001129,141,0,22.082400000010693,"2011-03-19",40621.60517361111,5.8,"I",420,"建屋東壁面","汚れ","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",3.5,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",9.74]
["MG05-7","仙台市南蒲生浄化センター",38,14,51.36,141,0,14.64,"2011-03-19",40621.62883101852,4.1,"I",410,"危険物conタンク","汚れ","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2.7,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",7.24]
["MG05-8","仙台市南蒲生浄化センター",38,14,50.1,141,0,15.37,"2011-03-19",40621.634247685186,4.3,"I",380,"建屋西壁面","泥","B","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2.8,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",7.54]
["MG06","民家",38,14,56.774400000009564,140,59,1.0572000000456683,"2011-03-19",40621.652083333334,2.5,"I",2000,"民家壁面","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",4.94]
["MG07","畑",38,15,8.679600000007781,140,57,57.283200000010766,"2011-03-19",40621.66332175926,0,"I",3510,"畑","地面模様・ヒアリング","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",2.44]
["MG08","多賀城市水道施設",38,15,7.196399999992309,140,58,14.584800000018276,"2011-03-19",40621.67282407408,0.8,"I",3100,"田圃の中の施設外縁フェンス","泥汚れ？","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",3,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",4.24]
["MG09","仙台市消防へリポート",38,13,44.605199999990646,140,59,7.267200000021603,"2011-03-19",40621.69449074074,1.8,"I",720,"格納庫ガラス面","草混じり泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",4.6,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",6.84]
["MG10-1","仙台市海岸公園センターハウス",38,13,21.19,140,59,8.49,"2011-03-19","17:04:00",2.5,"I",360,"内部前面に離岸堤有り","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1.6,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",4.54]
["MG10-2","仙台市海岸公園トイレ",38,13,21.09,140,59,10.4,"2011-03-19","17:04:00",1.7,"I",303,"建屋西壁面、遠景目視","汚れ","D","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1.6,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.7399999999999998]
["MG11-01","JA亘理町荒浜機械",38,3,38.04,140,54,7.67,"2011-03-20","09:42:00",2.4,"I",2410,"格納庫シャッター","泥うちあげ","A","国総研","河川からの越流の可能性あり",3,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",5.840000000000001]
["MG11-02","JA亘理町荒浜麦乾燥施設",38,3,38.58,140,54,7.71,"2011-03-20","09:43:00",1.7,"I",2390,"施設の窓ガラス","泥","A","国総研","河川からの越流の可能性あり",3,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",5.140000000000001]
["MG11-03","JA亘理町荒浜水稲育苗施設",38,3,36.56,140,54,6.75,"2011-03-20","09:46:00",1.2,"R",2405,"ビニールハウスの前面","泥","A","国総研","河川からの越流の可能性あり",2,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.64]
["MG12","水田横道路",38,4,2.2800000000108867,140,53,49.98120000004292,"2011-03-20","10:07:00",0.5,"I",3356,"ガードレール支柱","泥","A","国総研","河川からの越流の可能性あり",3,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.94]
["MG13-01","水田横道路",38,3,26.881200000009358,140,54,56.87999999996464,"2011-03-20","10:22:00",2.6,"I",654,"電柱","草","B","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",0.5,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.54]
["MG13-02","水田横道路",38,3,26.34119999999143,140,54,58.97879999998622,"2011-03-20","10:23:00",2.6,"I",603,"電柱","泥","B","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",0.1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.14]
["MG14-1","貞山堀　しんはま橋",38,3,25.441200000012714,140,55,10.441200000002482,"2011-03-20","10:27:00",3.4,"R",319,"松の木","松の枝折れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2.6,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",6.44]
["MG14-2","貞山堀　しんはま橋",38,3,21.240000000004216,140,55,9.001199999954679,"2011-03-20","10:31:00",4.8,"R",346,"松の木","松の枝折れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2.5,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",7.74]
["MG15-1","阿武隈川河口左岸",38,3,4.500000000011255,140,55,18.660000000022592,"2011-03-20","10:52:00",3.2,"R",78,"松の木","松の枝折れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",6.7,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",10.34]
["MG15-2","阿武隈川河口左岸",38,30,46.188000000029206,140,55,18.54120000001558,"2011-03-20","10:52:00",2.9,"R",81,"松の木","松の枝折れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",6.6,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",9.94]
["MG15-3","阿武隈川河口左岸",38,3,6.541199999999208,140,55,13.861199999962537,"2011-03-20","11:19:00",4.2,"R",202,"松の木","松の枝折れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1.6,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",6.240000000000001]
["MG15-4","阿武隈川河口左岸",38,3,6.660000000006221,140,55,15.481199999965156,"2011-03-20","11:23:00",4.2,"R",161,"松の木","松の枝折れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1.9,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",6.54]
["MG15-5","阿武隈川河口左岸",38,3,6.119999999988295,140,55,16.31999999999607,"2011-03-20","11:46:00",3.2,"R",209,"松の木","松の枝折れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1.9,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",5.54]
["MG15-6","阿武隈川河口左岸",38,3,6.4188000000012835,140,55,12.900000000036016,"2011-03-20","11:40:00",3.8,"R",223,"松の木","松の枝折れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1.6,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",5.840000000000001]
["MG16-1","海岸堤防破堤部背後",38,3,51.23880000000554,140,55,20.758800000044175,"2011-03-20","13:03:00",4,"I",139,"電柱","汚れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2.4,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",6.840000000000001]
["MG16-2","海岸堤防破堤部背後",38,4,3.6588000000085685,140,55,18.660000000022592,"2011-03-20","13:08:00",2.6,"R",219,"建物の壁","松の枝","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2.6,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",5.640000000000001]
["MG16-3","海岸堤防破堤部背後",38,4,2.8200000000032333,140,55,19.441199999994296,"2011-03-20","13:14:00",2.6,"R",199,"松の木","松の枝折れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1.1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",4.140000000000001]
["MG16-4","海岸堤防破堤部背後",38,4,2.5211999999902446,140,55,19.318799999996372,"2011-03-20","13:14:00",4.4,"R",202,"松の木","松の枝折れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1.1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",5.94]
["MG17","水田横道路",38,4,1.981199999997898,140,55,19.318799999996372,"2011-03-20","13:41:00",2.4,"I",1319,"電柱","汚れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",0.8,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.64]
["MG18","海岸堤防破堤部背後保安林",38,5,40.08120000000588,140,55,41.09879999995201,"2011-03-20","13:52:00",4.2,"R",117,"松の木","漂流物（布団）","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2.4,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",7.04]
["MG19","海岸堤防破堤部背後保安林",38,6,4.258799999996086,140,55,45.59880000005023,"2011-03-20","14:31:00",4.8,"R",137,"松の木","漂流物（浮き）","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",7.24]
["MG20","名取川河口左岸",38,10,55.9200000000061,140,57,29.941199999977925,"2011-03-20","15:34:00",4.6,"R",503,"松の木","松の枝折れ","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2.3,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",7.34]
["MG21","磯浜①",37,54,7.7,140,55,35,"2011-03-19","13:32:00",7.5,"I",164,"松の木","松の枝折れ","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",8.94]
["MG22","磯浜②",37,54,5.6,140,55,26,"2011-03-19","13:14:00",7.4,"I",383,"鉄塔","鉄塔の損傷","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",3,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",10.84]
["MG23","中浜",37,54,23.76,140,55,21.26,"2011-03-19","14:19:00",8.1,"I",184,"排水機場","屋根の損傷","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",5,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",13.54]
["MG24","坂元川水門",37,55,45.92,140,55,10.02,"2011-03-19","16:50:00",11.6,"I",135,"水門","水門建屋の損傷","A","国総研","海面からの高さ",0.36,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",12.399999999999999]
["MG25","坂元駅",37,55,41.7,140,54,45.94,"2011-03-19","17:26:00",6.4,"I",725,"跨線橋","窓ガラスの損傷","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",8.84]
["MG26","山下①",37,58,17.17,140,52,59.24,"2011-03-20","08:56:00",0,"R",2744,"田んぼの遡上先端","浸水痕跡","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",3,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.44]
["MG27","山下②",37,58,0.85,140,53,23.47,"2011-03-20","09:04:00",1,"I",2170,"建物","泥","A","国総研","道路からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",2,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",3.44]
["MG28","山下③",37,58,55.29,140,53,46.85,"2011-03-20","09:20:00",2,"I",1532,"家屋","泥","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",4,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",6.44]
["MG29","山下④",37,58,33.65,140,54,15.76,"2011-03-20","09:33:00",3.5,"I",864,"建物（コメリ）","壁の損傷","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",4,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",7.94]
["MG30","花釜",37,58,15.35,140,54,42.68,"2011-03-20","10:02:00",8.6,"I",232,"松の木","松の枝折れ","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",5,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",14.04]
["MG31","牛橋水門",37,59,21.88,140,54,49.83,"2011-03-20","11:14:00",10.8,"I",0,"水門","水門建屋の損傷","A","国総研","海面からの高さ",-0.51,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",10.73]
["MG32","吉田浜",38,0,2.89,140,54,46.86,"2011-03-20","10:32:00",7.3,"I",143,"松の木","松の枝折れ","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",5,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",12.74]
["MG33","荒浜①",38,2,19.77,140,54,58.54,"2011-03-20","12:12:00",5.5,"I",524,"建物","壁の損傷","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",1,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",6.94]
["MG34","荒浜②",38,2,25.33,140,55,14.77,"2011-03-20","12:22:00",6.4,"I",125,"松の木","松の枝折れ","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",5,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",11.84]
["MG35","蒲崎し尿処理場①",38,4,58.59,140,55,24.67,"2011-03-20","13:37:00",3.5,"I",299,"松の木","幹の傷","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",8,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",11.94]
["MG36","蒲崎し尿処理場②",38,4,57.55,140,55,26.43,"2011-03-20","13:34:00",4,"I",253,"松の木","幹の傷","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",7,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",11.44]
["MG37","蒲崎し尿処理場③",38,4,59.2,140,55,29.56,"2011-03-20","12:57:00",8.5,"I",185,"建物","壁の損傷","C","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",6,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",14.94]
["MG38","県南浄化センター①",38,6,35.97,140,55,34.82,"2011-03-20","14:38:00",3.8,"I",652,"松の木","松の枝折れ","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",4,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",8.24]
["MG39","県南浄化センター②",38,6,40.75,140,55,47.61,"2011-03-20","14:28:00",4.7,"I",403,"建物","ゴミ","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",5,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",10.139999999999999]
["MG40","県南浄化センター③",38,6,39.69,140,55,49.39,"2011-03-20","14:25:00",6,"I",349,"松の木","松の枝折れ","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",5,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",11.44]
["MG41","岩沼海浜緑地公園",38,7,1.77,140,55,53.73,"2011-03-20","15:25:00",8.9,"I",383,"展望台の盛土","ゴミ","A","国総研","地面からの高さ（「測定時の潮位」欄には測定点の地盤標高を記載）",4,"2011-03-11","15:30:00",-0.44,"港橋（塩釜）",13.34]
[]
[{"$nulls":16},"氏　名","所　属"]
[{"$nulls":16},"諏訪義雄","国土交通省国土技術政策総合研究所海岸研究室"]
[{"$nulls":16},"加藤史訓","国土交通省国土技術政策総合研究所海岸研究室"]
[{"$nulls":16},"野口賢二","国土交通省国土技術政策総合研究所海岸研究室"]
[{"$nulls":16},"渡邊国広","国土交通省国土技術政策総合研究所海岸研究室"]
[{"$nulls":16},"土屋修一","国土交通省国土技術政策総合研究所水資源研究室"]
{"$rows_empty":17}
[{"$nulls":16},"※代表者の氏名に◯を付ける．"]