{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["調査結果"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"調査結果","index":0,"n_rows":52,"n_cols":24,"rows_kept":52,"cut":false,"hidden":false,"merged":[[1,19,1,20],[0,16,2,16],[0,17,2,17],[0,18,0,23],[0,0,2,0],[0,1,0,15],[1,1,2,1],[1,2,1,4],[1,5,1,7],[1,8,2,8],[1,9,2,9],[1,13,2,13],[1,14,2,14],[1,15,2,15]],"flags":["formulas_cached_only"]}
["地点番号","現地調査",{"$nulls":14},"調査グループ","備考","潮位補正"]
[null,"地名","北緯",null,null,"東経",null,null,"年/月/日","時刻","測定高","津波高","汀線からの","測定対象","根拠","信頼度*2",null,null,"測定時の","最大波発生日時（予想）",null,"最大波発生時（予想）","潮位補正の","潮位補正後の高さ"]
[null,null,"度","分","秒","度","分","秒",null,null," a (m)","の種類*1","測定距離 (m)",{"$nulls":5},"潮位 b (m)","年/月/日","時刻","の潮位 c (m)","参照地点","a+b-c (m)"]
["T001","宮城県塩釜市寒風沢島",38,19,54.29954,141,7,24.7555,"2015-05-03","10:04:36",1.992,"I",null,"木の漂着物","遡上痕","A","千葉工大・東北大","Promark3による計測（すべて）"]
["T002","宮城県塩釜市寒風沢島",38,20,3.02564,141,7,16.15928,"2015-05-03","10:21:40",6.9,"R",null,"ワラなど","遡上痕","A","千葉工大・東北大"]
["T003","宮城県塩釜市寒風沢島",38,20,2.87588,141,7,17.78647,"2015-05-03","10:36:50",5.427,"R",null,"ワラなど","遡上痕","A","千葉工大・東北大"]
["T004","宮城県塩釜市寒風沢島",38,20,1.609,141,7,24.48738,"2015-05-03","11:10:11",4.582,"I",null,"電柱のアミ","遡上痕","A","千葉工大・東北大"]
["T005","宮城県塩釜市寒風沢島",38,20,0.44218,141,7,25.00345,"2015-05-03","11:27:51",6.088,"R",null,"植物の枯渇，ワラ","遡上痕","A","千葉工大・東北大"]
["T006","宮城県塩釜市寒風沢島",38,19,58.1005,141,7,28.30472,"2015-05-03","11:43:38",5.932,"R",null,"ワラなど","遡上痕","A","千葉工大・東北大"]
["T007","宮城県塩釜市寒風沢島",38,19,58.29085,141,7,29.52985,"2015-05-03","11:53:32",7.847,"I",null,"木の漂着物","遡上痕","B","千葉工大・東北大"]
{"$rows_empty":18}
["*1 津波高の種類",{"$nulls":15},"氏　名","所　属"]
["　　R: 遡上高",{"$nulls":15},"後藤和久","千葉工業大学"]
["　　I: 浸水深",{"$nulls":15},"菅原大助","東北大学"]
["　　P: 港内津波高（港湾において，岸壁は越えてはいないが明確に高さが分かる津波）",{"$nulls":15},"川俣秀樹","パシフィックコンサルタンツ"]
["　　W: 微弱な津波（常時波浪との判別が不可能な微弱な津波）"]
["*2 信頼度の判断基準"]
["　　A: 信頼度大なるもの。痕跡明瞭にして，測量誤差最も小なるもの。"]
["　　B: 信頼度中なるもの。痕跡不明につき，聞き込みにより，周囲の状況から信頼ある水位を知るもの。測量誤差小。"]
["　　C: 信頼度小なるもの。その他砂浜などで異常に波がはい上がったと思われるもの，あるいは測点が海辺より離れ測量誤差が大なるもの。"]
["　　D: 信頼度極小なるもの。高潮，台風などの影響で痕跡が重複し，不明瞭なもの，等。"]
{"$rows_empty":13}
[{"$nulls":16},"※代表者の氏名に◯を付ける．"]