{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["調査結果"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"調査結果","index":0,"n_rows":9,"n_cols":24,"rows_kept":9,"cut":false,"hidden":false,"merged":[[0,0,2,0],[0,1,0,15],[1,1,2,1],[1,2,1,4],[1,5,1,7],[1,8,2,8],[1,9,2,9],[1,13,2,13],[1,14,2,14],[1,15,2,15],[1,19,1,20],[0,16,2,16],[0,17,2,17],[0,18,0,23]],"flags":["formulas_cached_only"]}
["地点番号","現地調査",{"$nulls":14},"調査グループ","備考","潮位補正"]
[null,"地名","北緯",null,null,"東経",null,null,"年/月/日","時刻","測定高","津波高","汀線からの","測定対象","根拠","信頼度*2",null,null,"測定時の","最大波発生日時（予想）",null,"最大波発生時（予想）","潮位補正の","潮位補正後の高さ"]
[null,null,"度","分","秒","度","分","秒",null,null," a (m)","の種類*1","測定距離 (m)",{"$nulls":5},"潮位 b (cm)","年/月/日","時刻","の潮位 c (cm)","参照地点","a+b-c (m)"]
["Iw1","岩手県宮古市田老町小堀内・小堀内漁港（グリーンピア田老の東方海岸）",39,47,20.28,141,58,58.2,"2015-04-04","13:29:00",37.38,"Ｒ",null,"自動車道路から山道の50mのど昇った地点。木片漂流物、および雑草流跡より判定","漂流物＋雑草流跡","B","東大地震研",null,2,"2011-03-11","15:06:00",-50,"宮古",37.88]
["Iw2","岩手県宮古市田老町田老漁港出羽神社前階段坂",39,44,12.02,141,58,41.23,"2015-04-04","15:10:00",18.6,"Ｒ",null,"石段上端から神社に至る路の西側の杉の木の根本","漂流物＋雑草流跡","B","東大地震研",null,24,"2011-03-11","15:06:00",-50,"宮古",19.1]
["Iw3","岩手県宮古市田老町三陸鉄道田老駅北方レール面（家材堆積物が載る）",39,44,4,141,58,0,"2015-04-04","16:50:00","TP11.678,MSL11.242","Ｒ",null,"三陸鉄道田老駅プラットホーム北方約200m付近で線路上に漂流家材が覆う。レール面をTP5.7水準点を起点として測量。","漂流物","B","東大地震研","TP基準標高から(a)MSL０の標高がTP０の標高より13.3㎝上方にあること（1996～2000年気象庁潮位表、宮古検潮所）、(b)今回の地震によって、この付近の地盤が約30cm沈下していると考えられること、(c）この付近の海岸での最大津波来襲時刻は地震後約20分の証言から15時06分頃と見られ、このときの潮位は-50cmであった。TP標高値から(a)、(b),（ｃ）の３個の数値を引き算して得た数値11.74ｍをここでの正味の津波による水位上昇量とする。","TP5.7水準点起点につき無意味","2011-03-11","15:06:00",-50,"宮古",11.74]
["Iw4","岩手県宮古市田老町青野滝漁港",39,46,17.39,141,59,10.2,"2015-04-05","11:23:00",34.27,"Ｒ",null,"港に降りる道路脇堆積物＋雑草流跡＋小浸食痕跡あり","雑草流跡","B","東大地震研",null,-59,"2011-03-11","15:06:00",-50,"宮古",34.77]
["Iw5","岩手県宮古市田老町田老第一中学校敷地内文化センター（遺体安置所）",39,44,18,141,58,10,"2015-04-04","17:30:00","TP12.5","Ｒ",null,"中学校グラウンドは浸水。敷地内文化センター遺体安置所に水位痕跡、グラウンド面より1.0m上方。同グラウンドの三角点は11.5m（TP)。(a)MSL０の標高がTP０の標高より13.3㎝上方にあること（1996～2000年気象庁潮位表、宮古検潮所）、(b)今回の地震によって、この付近の地盤が約30cm沈下していると考えられること、(c）この付近の海岸での最大津波来襲時刻は地震後約20分の証言から15時06分頃と見られ、このときの潮位は-50cmであった。TP標高値から(a)、(b),（ｃ）の３個の数値を引き算して得た数値11.74ｍをここでの正味の津波による水位上昇量とする。","水位痕跡","B","東大地震研","TP基準標高から(a)MSL０の標高がTP０の標高より13.3㎝上方にあること（1996～2000年気象庁潮位表、宮古検潮所）、(b)今回の地震によって、この付近の地盤が約30cm沈下していると考えられること、(c）この付近の海岸での最大津波来襲時刻は地震後約20分の証言から15時06分頃と見られ、このときの潮位は-50cmであった。TP標高値から(a)、(b),（ｃ）の３個の数値を引き算して得た数値11.74ｍをここでの正味の津波による水位上昇量とする。","三角点11.5m基準","2011-03-11","15:06:00",-50,"宮古",12.6]
[{"$nulls":11},"　",{"$nulls":5},"調査者：都司嘉宣、杉本めぐみ、泊次郎、大木聖子"]