{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["調査結果"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"調査結果","index":0,"n_rows":50,"n_cols":26,"rows_kept":50,"cut":false,"hidden":false,"merged":[[0,0,2,0],[0,1,0,15],[1,1,2,1],[1,2,1,4],[1,5,1,7],[1,8,2,8],[1,9,2,9],[1,13,2,13],[1,14,2,14],[1,15,2,15],[1,19,1,20],[0,16,2,16],[0,17,2,17],[0,18,0,23]],"flags":["formulas_cached_only"]}
["地点番号","現地調査",{"$nulls":14},"調査グループ","備考","tyouihosei "]
[null,"地名","北緯",null,null,"東経",null,null,"年/月/日","時刻","測定高","津波高","汀線からの","測定対象","根拠","信頼度*2",null,null,"測定時の","最大波発生日時（予想）",null,"最大波発生時（予想）","潮位補正の","潮位補正後の高さ","標高を基準とした","潮位補正後の高さ"]
[null,null,"度","分","秒","度","分","秒",null,null," a (m)","の種類*1","測定距離 (m)",{"$nulls":5},"潮位 b (m)\n標高","年/月/日","時刻","の潮位 c'(m)\n標高","参照地点","a+b-c (m)\n標高","潮位表基準面との差d（m）","a+b-c+d (m)\n潮位表基準面"]
[3,"岩手県宮古市田老町田老漁港",39,44,18,141,58,21.9,"2011-04-15","12:57:00",7.09,"R",null,"ビルの壁","浸水痕","A","港空研",null,0.22,"2011-03-11",null,-0.46,"宮古",7.77,0.81,8.58]
[4,"岩手県宮古市田老町三王遊歩道",39,44,0.4,141,58,46.5,"2011-04-15","14:48:00",28.23,"R",null,"崖の遡上先端","浸水痕","A","港空研",null,0.12,"2011-03-11",null,-0.46,"宮古",28.810000000000002,0.81,29.62]
[5,"岩手県宮古市田老町樫内漁港",39,42,23.6,141,58,29.4,"2011-04-15","17:19:00",21.07,"R",null,"山の遡上先端","浸水痕","A","港空研",null,-0.29,"2011-03-11",null,-0.46,"宮古",21.240000000000002,0.81,22.05]
[7,"岩手県宮古市太田ノ浜",39,36,5,141,58,19.4,"2011-04-16","08:42:00",8.52,"R",null,"山の遡上先端","浸水痕（漂流物）","A","港空研",null,-0.47,"2011-03-11",null,-0.46,"宮古",8.51,0.81,9.32]
[8,"岩手県宮古市太田ノ浜",39,36,24,141,58,31.9,"2011-04-16","09:02:00",16.67,"R",null,"山の遡上先端","浸水痕（漂流物）","A","港空研",null,-0.46,"2011-03-11",null,-0.46,"宮古",16.67,0.81,17.48]
[9,"岩手県宮古市重茂",39,36,8,142,1,32,"2011-04-16","10:12:00",25.91,"R",null,"道路上の木くず","浸水痕（漂流物）","A","港空研",null,-0.29,"2011-03-11",null,-0.46,"宮古",26.080000000000002,0.81,26.89]
[10,"岩手県宮古市重茂鵜磯小学校",39,36,58.5,142,1,8.7,"2011-04-16","10:48:00",26.03,"R",null,"倉庫の壁","浸水痕","A","港空研",null,-0.18,"2011-03-11",null,-0.46,"宮古",26.310000000000002,0.81,27.12]
[11,"岩手県宮古市重茂仲組漁港立浜地区",39,38,8.4,142,1,16,"2011-04-16","11:26:00",19.09,"R",null,"山の遡上先端","浸水痕（漂流物）","A","港空研",null,-0.05,"2011-03-11",null,-0.46,"宮古",19.5,0.81,20.31]
{"$rows_empty":15}
["*1 津波高の種類",{"$nulls":15},"氏　名","所　属"]
["　　R: 遡上高",{"$nulls":15},"○有川　太郎","耐波研究チーム"]
["　　I: 浸水深",{"$nulls":15},"佐藤　昌治","耐波研究チーム"]
["　　P: 港内津波高（港湾において，岸壁は越えてはいないが明確に高さが分かる津波）",{"$nulls":15},"鷲崎　誠","耐波研究チーム"]
["　　W: 微弱な津波（常時波浪との判別が不可能な微弱な津波）"]
["*2 信頼度の判断基準"]
["　　A: 信頼度大なるもの。痕跡明瞭にして，測量誤差最も小なるもの。"]
["　　B: 信頼度中なるもの。痕跡不明につき，聞き込みにより，周囲の状況から信頼ある水位を知るもの。測量誤差小。"]
["　　C: 信頼度小なるもの。その他砂浜などで異常に波がはい上がったと思われるもの，あるいは測点が海辺より離れ測量誤差が大なるもの。"]
["　　D: 信頼度極小なるもの。高潮，台風などの影響で痕跡が重複し，不明瞭なもの，等。"]
{"$rows_empty":13}
[{"$nulls":16},"※代表者の氏名に◯を付ける．"]