{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["調査結果"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"調査結果","index":0,"n_rows":48,"n_cols":26,"rows_kept":48,"cut":false,"hidden":false,"merged":[[1,9,2,9],[1,13,2,13],[1,14,2,14],[1,15,2,15],[1,19,1,20],[0,16,2,16],[0,17,2,17],[0,18,0,23],[0,0,2,0],[0,1,0,15],[1,1,2,1],[1,2,1,4],[1,5,1,7],[1,8,2,8]],"flags":["formulas_cached_only"]}
["地点番号","現地調査",{"$nulls":14},"調査グループ","備考","潮位補正"]
[null,"地名","北緯",null,null,"東経",null,null,"年/月/日","時刻","測定高","津波高","汀線からの","測定対象","根拠","信頼度*2",null,null,"測定時の","最大波発生日時（予想）",null,"最大波発生時（予想）","潮位補正の","潮位補正後の高さ"]
[null,null,"度","分","秒","度","分","秒",null,null," a (m)","の種類*1","測定距離 (m)",{"$nulls":5},"潮位 b (m)","年/月/日","時刻","の潮位 c (m)","参照地点","a+b-c (m)",null,"T.P.基準の測定高"]
[1,"千葉県船橋漁港",35,41,23.7,139,59,1.3,"2011-03-20","13:12:00",3.01,"I",null,"港内倉庫外壁のwater mark","周辺にも同様の痕跡有り．目撃証言あり","A","横国大・大成建設",null,-0.4,{"$nulls":6},2.61]
[2,"千葉県船橋漁港",35,41,25.1,139,59,2,"2011-03-20","13:12:00",2.79,"I",null,"港内倉庫外壁のwater mark","周辺にも同様の痕跡有り．目撃証言あり","A","横国大・大成建設",null,-0.4,{"$nulls":6},2.39]
[3,"千葉県船橋漁港",35,41,21.5,139,58,59.6,"2011-03-20","13:40:00",2.83,"I",null,"漁港陸上ゲートのwater mark","周辺にも同様の痕跡有り．目撃証言あり","A","横国大・大成建設","船橋漁港の陸上ゲートは閉鎖され，漁港外への浸水無し",-0.19,{"$nulls":6},2.64]
[4,"千葉県船橋漁港",35,41,27,139,59,6.7,"2011-03-20","13:55:00",2.54,"I",null,"港内倉庫外壁のwater mark","周辺にも同様の痕跡有り．目撃証言あり","A","横国大・大成建設",null,-0.06,{"$nulls":6},2.48]
[5,"千葉県木更津港",35,22,53.8,139,54,54.6,"2011-03-20","15:55:00",1.33,"R",null,"厚生水産（商店）入り口の地盤高","目撃証言あり","B","横国大・大成建設","内水氾濫であり，岸壁は越流しておらず，側溝から水が溢れた（証言）．岸壁パラペットの高さはT.P.+2.4m",0.61,{"$nulls":6},1.94]
[6,"千葉県木更津漁港あづま",35,23,18.2,139,55,6.5,"2011-03-20","16:40:00",1.52,"I",null,"アサリ加工場建屋外壁のwater mark","目撃証言あり","A","横国大・大成建設","建屋入り口のシャッター下部が水圧で破損",0.8,{"$nulls":6},2.32]
{"$rows_empty":15}
["*1 津波高の種類",{"$nulls":15},"氏　名","所　属"]
["　　R: 遡上高",{"$nulls":15},"○佐々木 淳","横浜国立大学"]
["　　I: 浸水高",{"$nulls":15},"伊藤 一教","大成建設(株)"]
["　　P: 港内津波高（港湾において，岸壁は越えてはいないが明確に高さが分かる津波）",{"$nulls":15},"高山 百合子","大成建設(株)"]
["　　W: 微弱な津波（常時波浪との判別が不可能な微弱な津波）",{"$nulls":15},"アグング ウィヨノ レトノ ウタミ*","横浜国立大学大学院"]
["*2 信頼度の判断基準"]
["　　A: 信頼度大なるもの。痕跡明瞭にして，測量誤差最も小なるもの。"]
["　　B: 信頼度中なるもの。痕跡不明につき，聞き込みにより，周囲の状況から信頼ある水位を知るもの。測量誤差小。"]
["　　C: 信頼度小なるもの。その他砂浜などで異常に波がはい上がったと思われるもの，あるいは測点が海辺より離れ測量誤差が大なるもの。"]
["　　D: 信頼度極小なるもの。高潮，台風などの影響で痕跡が重複し，不明瞭なもの，等。"]
{"$rows_empty":13}
[{"$nulls":16},"※代表者の氏名に◯を付ける．"]