{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"sheet1","index":0,"n_rows":55,"n_cols":24,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,0,2,0],[0,1,0,15],[0,16,2,16],[0,17,2,17],[1,13,2,13],[1,14,2,14],[1,15,2,15],[0,18,0,23],[1,1,2,1],[1,2,1,4],[1,5,1,7],[1,8,2,8],[1,9,2,9],[1,19,1,20]],"flags":["formulas_cached_only"]}
["地点番号","現地調査",{"$nulls":14},"調査グループ","備考","潮位補正"]
[null,"地名","北緯",null,null,"東経",null,null,"年/月/日","時刻","測定高","津波高","汀線からの","測定対象","根拠","信頼度*2",null,null,"測定時の","最大波発生日時（予想）",null,"最大波発生時（予想）","潮位補正の","潮位補正後の高さ"]
[null,null,"度","分","秒","度","分","秒",null,null," a (m)","の種類*1","測定距離 (m)",{"$nulls":5},"潮位 b (m)","年/月/日","時刻","の潮位 c (m)","参照地点","a+b-c (m)"]
[1,"松川浦",37,49,24.31,140,58,45.42,"2011-05-01","16:59:00",15.45,"R",220,"枝にかかった海藻","同じ高さに複数の漂流物も見られた","A","東大"]
[131,"志津川湾波伝谷",38,38,47.5,141,27,55.3,"2011-05-02","12:57:00",14.31,"R",70,"枝にかかった海藻","同じ高さに複数の漂流物も見られた","A","東大"]
[132,"志津川湾津の宮",38,38,27.2,141,29,7.3,"2011-05-02","13:23:00",12.46,"I",70,"家屋の窓に浸水痕","目撃証言","A","東大"]
[133,"志津川湾藤浜",38,38,14.2,141,30,10.7,"2011-05-02","13:54:00",13.84,"R",118,"家屋の雨どいに漂流物","同じ高さに複数の漂流物も見られた","A","東大"]
[135,"志津川湾長清水",38,38,9.3,141,30,39.1,"2011-05-02","14:10:00",10.15,"I",57,"斜面上の漂流物","同じ高さに複数の漂流物も見られた","A","東大","奥に深い低平地を囲む斜面の海側での痕跡"]
[137,"志津川湾寺浜",38,38,11.4,141,31,15.7,"2011-05-02","14:24:00",12.16,"R",110,"斜面上の漂流物","同じ高さに複数の漂流物も見られた","A","東大"]
{"$rows_empty":22}
["*1 津波高の種類",{"$nulls":15},"氏　名","所　属"]
["　　R: 遡上高",{"$nulls":15},"田島芳満","東京大"]
["　　I: 浸水深",{"$nulls":15},"関口","東京大(学生)"]
["　　P: 港内津波高（港湾において，岸壁は越えてはいないが明確に高さが分かる津波）",{"$nulls":15},"佐々木","東京大(学生)"]
["　　W: 微弱な津波（常時波浪との判別が不可能な微弱な津波）"]
["*2 信頼度の判断基準"]
["　　A: 信頼度大なるもの。痕跡明瞭にして，測量誤差最も小なるもの。"]
["　　B: 信頼度中なるもの。痕跡不明につき，聞き込みにより，周囲の状況から信頼ある水位を知るもの。測量誤差小。"]
["　　C: 信頼度小なるもの。その他砂浜などで異常に波がはい上がったと思われるもの，あるいは測点が海辺より離れ測量誤差が大なるもの。"]
["　　D: 信頼度極小なるもの。高潮，台風などの影響で痕跡が重複し，不明瞭なもの，等。"]
{"$rows_empty":13}
[{"$nulls":16},"※代表者の氏名に◯を付ける．"]